# NAO Chair Plan (wood)

Dave Snowdon

v0.2

# Introduction

This prototype used 15mm sheets of wood (plywood except for the armrests). This thickness is not necessary for structural strength or rigidity and the design should work as well with plywood of as little as 5mm. However, if wood of a different thickness is used then some of the measurements will need to be adjusted.

# Front elevation

# Side elevation

# Top elevation

# Cut list

1 x back

2 x side

1 x seat

2 x arm rest

1 x stabliser (at back)